## Changelog Version 2.1.1.0

### Changed

- Supporting firmware updates for TN-UHF-Q300-LNX and TN-UHF-Q180L300-LNX in the Network View
- Supporting of CMVT-M8TE1X-LI2IOL-H1141 in the vibration monitor

### Fixed

- Activated license can be lost after some days
- Issue with login on devices with default address
- Set the process output as long as the window is open or until they are changed by the PLC, etc.

## Changelog Version 2.1.0.0

### Added

- Unlimited use (24/7) of the TAS Edge IoT Service for collecting IO-Link data and forwarding it to an MQTT broker, TAS Cloud, and AWS
- License activation:
  - License activation for the TAS Edge IoT Service on TX devices for unlimited use (24/7) via TAS license ID
  - License activation for the TAS Edge IoT Service on a PC for unlimited use (24/7) via TAS license ID
  - Download CodeMeter Runtime for license activation
- TAS Edge user management:
  - Includes user management view
  - Control over access rights for the device network and the TAS Edge configuration
  - Display & use of users from the TURCK HMI device (TX)
  - Extend and customize user roles
- TAS Edge Gateway View:
  - Topology scan for compatible devices
  - Install TAS Edge, CodeMeter Runtime, and the TAS Cloud Connector on the target device via an action button and enable the app’s auto-start
  - Display devices, version, and status of installed apps
  - Time synchronization of TX devices can be executed as an action
  - Executing updates for TAS Edge
  - Opening the TAS Edge user interface in the local web browser from a PC
- TAS Edge on TX supports a direct connection to the TAS Cloud without the TAS Cloud Connector
- Teach Monitor for the new FS501 flow measuring sensor:
  - to view the live flow and temperature process values changes against time
  - to view the different switching points of the configured switching outputs as per settings in single point, two point or window modes
  - Different color codes of the process values and outputs for easy identification
  - Do a single value teach or Dynamic Teach for the switching point in different units for flow velocity or volume flow and temperature as per the sensor configuration that enables easy integration and initial settings on the sensor.
- Expansion of the vibration monitor to include measurement start
  - Load vibration data via BLOB data transfer and display it as acceleration values over time
  - Load vibration data via BLOB data transfer and then perform an FFT (Fast Fourier Transform) to display the vibration in the frequency range
- Export all data
- Support for TBEN-L5-WR-PLUS
- Support for FEN20-16DXP-NEX

### Changed

- Updated Getting Started for TAS Edge IoT
- Improved usability when creating and configuring IoT templates:
  - Revised user guidance after saving IoT templates
  - Support for IO-Link parameters in IoT templates for data forwarding to an MQTT broker
  - Reduced number of MQTT topics by default, without menu and group names
  - New IoT templates are used by default during automatic device assignment
  - Data forwarding is enabled by default only for IO-Link process data
  - Wink in the IoT Edge and IoT1 device view for visual identification of the device
  - New parameter to set the polling rate of the MQTT preview
  - Read rate adjustable in batch mode
  - Limit the value range of the delta for digital data points to 0 and 1
  - Improvement of status information after activating data forwarding for IoT1 devices
  - Information rearranged in the IoT Template Views
- Reset of filters for the device network after a TAS restart
- Support for TAS Edge on TX devices starting with BSP 1.3
- Automatic redirection to the TX device’s HTTPS website
- Improved compatibility with the new IODD of IO-Link ring sensors
- Frontend optimizations when opened via a smartphone/tablet
- Adjustments to the RFID app Tag Population to display the RSSI value and expansion with new filters and export options
- Moving dialog windows
- Optimized TAS startup time
- Display of the TAS icon when TAS is launched
- Network scan is repeated only for changed devices
- Encryption of the database for TAS settings
- Improvements to the Bluetooth view by adding additional information and changes to the display of devices
- Visualize measured values in the Bluetooth view
- Button for the DHCP server made visible in the settings dialog
- Support for new event codes from IODD Spec. v1.1.5
- Block firmware updates if IP addresses in the network are identical
- Return to the last navigation point on the IO-Link device when accessed via the IO-Link view
- Reduction of device identification data, e.g., in the vibration monitor
- General optimizations and improvements

### Fixed

- Customized IoT templates cannot be applied in some cases
- Incorrect values are displayed in the IoT Edge View when editing the IoT template
- Setting the delta for data forwarding from a data point to the TAS Cloud does not work in certain cases
- Incorrect statuses during device assignment to the IoT template
- An empty topic prefix results in an error message
- Allow 32 characters in IO-Link application-specific tags
- Prevent modification of IO-Link process data only when the fieldbus is active
- IO-Link Enums in combination with input values
- IO-Link Enums with default values and gain/offset
- Value ranges in IO-Link Enums where the value is the default
- EPC list in the RFID app “Tag Population” is incorrect in some cases
- Error during firmware download to BLC devices
- Use of TX devices named “HMI”
- Incorrect overlapping of text and dialogs with certain browser window sizes
- Save changes to the Quick Connect status
- Device name in the TAS scan list may be displayed incorrectly in certain cases when a device is added manually
- Wait time after resetting to factory settings to load device information
- Text messages and tooltips have been updated
- General bug fixes

## Changelog Version 2.0.2.0

### Fixed

- Error when accessing certain IO-Link devices, such as the SD50 LED indicator light
- Incorrect values displayed when configuring data points

## Changelog Version 2.0.1.0

### Fixed

- The time required to scan for devices in the network has been optimized
- Firmware update for TBPN-… no longer blocked
- DP template configurations can be saved if the topics for deactivated datapoints have not been configured
- Display error in the table of the IO-Link function “Test Read/Write”
- Error when accessing TN-UHF-Q150-… via TAS
- Error when displaying the set power of the TN-UHF-Q150-…
- Display error in selection fields

## Changelog Version 2.0.0.0

### Added

- TAS Edge on TX devices:
  - Download TAS Edge IIoT Demo on TX to collect IO-Link data and forward it to an MQTT broker
  - Download TAS Edge IIoT Demo on TX to collect IO-Link data and forward it to the TAS Cloud via the TAS Cloud Connector
  - Execute TAS Desktop functions such as Network, ARGEE, BEEP, Diagnosis, IO-Link, IOT DP Template, and IOT Edge Views on a TX device in the network
- TAS Edge IIoT Demo for collecting IO-Link data and forwarding it to an MQTT broker from a PC
- TAS Edge IIoT Demo for collecting IO-Link data and forwarding it directly to the TAS Cloud from a PC
- IOT Edge View:
  - Topology scan for compatible devices
  - Automatic device assignment and prefilling of topics
  - Assign data point templates to IO-Link devices and configure and start data forwarding by TAS Edge
  - Assign topic names and define the data format and payload
  - Configure the MQTT connection or TAS Cloud connection, including encryption (TLS) with certificates, optional MQTT via WebSockets, and connection testing
  - Preview the topics and display the transmitted data when activated
  - Check the status of the MQTT connection and the IOT Edge service
- View for IOT1 I/O modules:
  - Assign data point templates to IO-Link devices and activate data forwarding from the MQTT master
  - Configuration of the MQTT connection including encryption (TLS)
  - Start and stop the MQTT communication
- Download TAS Cloud Connector on TX to connect to the TAS Cloud
- Open the configuration for the TAS Cloud Connector from the network view
- Teach monitor for level monitoring and precise adjustment of new-generation BC… & UC… capacitive sensors
- Motor monitor for visualizing process data and displaying information about motors connected to TBEN-LLx-4RMC
- Metal differentiation monitor for S950 inductive sensors
- Central settings dialog for executing TAS and selecting network adapters
- Support for BL20-EL-GW-EN
- Support for TBEN…-IOT1 devices
- Password support for TBEN…-SE-…
- Language switching from Japanese

### Changed

- IOT DP template view:
  - Topology scan for compatible devices
  - Definition of default templates for automatic device assignment
  - Online and offline configuration of data forwarding for individual data points
  - Configuration of the read rate and continuous data forwarding in case of changes by TAS Edge
  - Assignment of Postfix topics
- Temporary or static setting of the IP address
- Optimization of the scan for devices in the network
- Displays the polarization of the UHF antenna in the RFID Test and Tag Trace application
- Saving the preset power of the UHF antenna in the Tag Population application
- Adjustment of the HF data carrier numbering application
- New sorting order in the views
- The sorting order of the views is no longer lost when changing pages
- Display DHCP status in the network view
- The last port used is saved and used when TAS is restarted
- Adjustment of the dialog for firmware updates
- Update view and function for M12-Plus
- Update EULA
- General security improvements
- Improved display at different screen resolutions
- General optimizations and improvements to user-friendliness

### Fixed

- Display message if JavaScript is not enabled in the web browser
- Missing network parameters for certain I/O modules
- Compatibility with factory reset of TX devices
- Error in web server documentation regarding Ethernet IP mapping
- Support for firmware updates for TBEN…-CDS-WV devices
- Error when creating a backup of the CODESYS application
- Compatibility of the USB IO-Link master
- Fieldbus communication disruptions caused by the IO-Link web part or when creating the diagnostic report
- Error in batch function for changing passwords on the Turck Switch
- Error when calling up the diagnostics of the FEN20-4DI-4DXP
- Error during batch firmware update
- Table filter set via web browser
- Freezing of the visualization with the TBEN-S2-4AI
- Error during firmware download of the TN-UHF-Q300-…-LNX
- Display of input/output data for certain RFID interfaces
- Display of manually added devices when changing views
- Firmware update for Excom I/O discs
- Some text messages and tooltips updated
- General bug fixing

## Changelog Version 1.12.1.0

### Fixed

- Missing update option in TAS
- Missing notification of new TAS versions
- Blocked actions on certain devices

## Changelog Version 1.12.0.0

### Added

- Introduction of the “PN Tag Location” for clear assignment of the devices to the location/machine
  - Writing the "PN Tag Location" via Edit device in the Network View
  - Reading and displaying the "PN Tag Location" in all views
  - "PN Tag Location" added to the device website
- Support of the following functions for the Turck Switch:
  - User and password query
  - Firmware updates
  - Editing the device settings
  - Reset options
- Data points view / configuration MQTT for IO-Link :
  - Create and save DP templates from the monitoring and diagnostic dialogs
  - Select DP templates
  - Open connection settings dialog
  - Export DP templates including connection settings
  - Download data forwarding configuration in IO-Link master
- Firmware download in CODESYS view
- Filter option in network view
- The EPCs in the UHF demo and test applications can be sorted
- A user can be defined for the global password that is used when logging in to the device (if required)
- Automatic update of displaying the USB-2-IOL-0002
- TAS Readme extended to include TAS start parameters and error handling
- Additional query in PROFINET View before resetting devices

### Changed

- New design and dialogs for the network view
- Loading status for the device data is displayed while loaded information is already visible
- The message that the firewall has been automatically configured disappears automatically after 3 seconds and TAS starts
- The current password is no longer requested when changing it if the user is logged in
- Improved error descriptions if TAS does not start
- The "Edit device" function can be activated for 180 seconds after a power reset on the device and can be changed without a password prompt, e.g. to change the IP address.
- Improvement of the import of parameters for stations
- Download of the IODD via additional link in the web part of the IO-Link device
- Improvement when importing IODD parameters
- Adjusted scaling for radar sensors
- Display CODESYS program version, even if the user administration is inactive
- Restore CODESYS applications without manual stop
- Inform when a CODESYS application with a different name is imported
- Adjustment of scaling in the vibration monitor
- Slider for setting the UHF configuration removed
- Adjustment of the output in the log file
- Adjustment of various icons and texts
- Adjustments to the website layout
- General improvements

### Fixed

- Compatible with older device versions to perform a firmware update, reset a device or adjust the device settings
- Compatible with certain versions of the USB-2-IOL-0002
- Information from manually added devices is updated when scanning
- Check whether the port is blocked by an already running TAS instance
- Error when downloading ARGEE projects
- Error when loading the IODD for an SD50 LED indicator light
- Error when switching off the Wink in the BEEP network
- Error when firmware download of certain devices was not possible in TAS
- Error when actions were temporarily deactivated
- Error where firmware download of certain devices via the website in TAS was not possible
- Error where actions were temporarily disabled
- Error in the display after shrinking and enlarging the web browser window
- More precise configuration of cable attenuation and antenna gain for an external UHF antenna
- Some text messages and tooltips updated

## Changelog Version 1.11.1.0

### Fixed

- Prevents the connected devices from detecting address conflicts after only the PROFINET station name has been set.

## Changelog Version 1.11.0.0

### Added

- RFID tag actions UHF:
  - Scans EPCs of UHF tags and creates a list
  - Reads tag memory in Hex and ASCII
  - Edits data and writes it to the tag in Hex
  - Places specific data in the entire or a selected memory area of the tag
  - Multitag support
  - Selection of the memory area
- Numbering of HF data carriers:
  - Numbering of data carriers from start value, according to counting step/increment size and data format
  - The data carriers are processed in sequence and the user area is written and added to the table with UID and value
- Editor for generic IO-Link access
- Supports Turck specific functions for backup and restore of the PlcLogic folder to backup and restore CODESYS applications
- Filter option in ARGEE and BEEP view
- Batch processing for restoring the CODESYS application according to the CODESYS standard function
- Setting of parameters via slider
- Data sheet of connected IO-Link devices can be called up

### Changed

- Renaming to TAS Desktop
- New design for the CODESYS view
- New design for the ARGEE view
- New design for the BEEP view
- Distinction between backup and restore of a CODESYS application according to the CODESYS standard function and the Turck-specific function
- Backup1 and Restore1 of a CODESYS application can be performed even if the CODESYS application has not been stopped
- Update for non-safe firmware of safety devices is supported
- Improved compatibility with certain IODDs
- Improved error handling when writing system commands for IO-Link
- Support for changing the COM port for the IO-Link light curtain
- No dependency on installed .Net Runtime versions
- A warning is issued if TAS is still open in a browser
- Feedback after downloading new updates from TAS
- Display of unknown unit codes in the IO-Link web part
- Display of enums/texts in diagrams
- Warning is issued if an IODD has been subsequently changed
- Forwarding to the device website if access via TAS is not possible
- TAS log file under Documentation
- Customization of the output in the log file
- Customization of various icons and texts
- Adjustments made to the website layout

### Fixed

- Improved stability when recognizing RFID readers
- CMVT-M8TA1X-LI2IOL-H114 support in the Vibration Monitor
- Backup of CODESYS application with date
- Correct drop-down menu for certain IO-Link devices
- Firmware download blocked for incompatible HF read/write heads
- Support for firmware updates for all available country variants of UHF readers
- Confirmation of the error message for the safety module corrected
- Export/import of parameter LED behavior (PWR) at V2 undervoltage in webpage corrected.
- No program crash when running multiple IO-Link USB masters
- No freezing of the diagram view in certain cases
- A device that is no longer available after updating the diagnostics is displayed in the diagnostics monitor
- Updated text messages and tooltips

## Changelog Version 1.10.0.0

### Added

- Profinet View & DCP (requires Npcap or Winpcap):

  - Scans and displays all DCP-enabled devices on the network
  - Identifies specific information about connected Profinet devices
  - Performs specific device actions:
    - Customizes IP Address, Profinet Device Name, Subnet Mask, Gateway
    - Different Reset Modes
    - Wink for visual identification

- Diagnose View:

  - Scans the Turck devices on the network and flags devices with existing diagnostics
  - Displays the device status or diagnostic message
  - Direct link to the creation of the diagnostic report
  - Accessing the detailed diagnostics page of the affected device

- Monitoring and visualization of EZ-Array light curtain with light beams that can be switched on and off.

- Optional: start of a DHCP server with the following functions

  - DHCP Scan List
  - DHCP Start/Stop
  - DHCP Get Adapter List

- Visualizes the time sequence of process input data of connected analog devices/sensors

- CODESYS recipes and/or log files (USB data) are uploaded to the PC

### Changed

- Automatic checking and display of new TAS versions
- The execution of TAS to set the firewall rules without administrator rights can be stopped without the TAS being executed
- Bar graphs for the display of the RFID tags in the read/write area and the detuning of the RF read/write head in the HF RFID tag actions
- IP 0.0.0.0 is treated as a default IP address in the network view
- For compatible IO-Link devices, the product variant ID or description ID is also displayed in the IO-Link Web Part when changing the DeviceID
- View IP address and Profinet device name when a device is opened via TAS
- An ARGEE project in the device can be overwritten via the ARGEE view without prior deletion if no protection is set
- Backup name of the CODESYS application is made up of the name of the CODESYS application, IP address and date
- Support for Q180/Q300-LNX UHF readers
- Customization of different icons and texts
- Adjustments to the website layout

### Fixed

- Malfunction due to CODESYS user login on certain firmware versions
- Compatibility problems with existing backups of the CODESYS application
- If more IODDs are linked than the memory size of the web browser allows, the oldest IODD is replaced
- Fixed Modbus TCP and EtherNet/IP™ memory mapping in web client
- Added missing channel numbers in Modbus TCP and EtherNet/IP™ memory mapping
- Display of BEEP support of the FEN20-4DIP-4DOP
- Incorrect sorting of IP addresses in IO-Link and CODESYS views
- Excom Gen: Failsafe mode is not displayed on all modules
- Updated some text messages and tooltips

## Changelog Version 1.9.1.0

### Changed

- Output of further messages in the CODESYS view
- Display of signal quality and antenna detuning only with compatible read/write heads
- FFT scaling in the Radar Monitor

### Fixed

- Missing ASCII characters in the HF tag actions
- Adjustment of the scrollbar
- Some text messages and tooltips updated
- Multiple display of the vibration monitor

## Changelog Version 1.9.0.0

### Added

- CODESYS View:
- Scans and displays all CODESYS devices on the network
  - Retrieves specific information about connected CODESYS devices
  - Performs specific device actions:
    - Saves application to CODESYS device (Restore 1)
    - Downloads application from CODESYS device (Backup 1)
    - Warm start of the application
    - Cold start the application
    - Stops the application
  - Supports CODESYS user and password handling
  - Save application to the device as a batch function
- Change language to Chinese, French or Spanish
- Cable Monitor for the M12Plus connector
- Vision Monitor for intelligent cameras
- Extension of the RFID tag actions HF to include visualization of signal quality and antenna detuning
- Extension of the RFID tag actions HF by the number of readings
- Manually added devices in the network view are also displayed in the BEEP, ARGEE and CODESYS view and actions can be performed
- Polling option to prevent resetting of the IO-Link process output data after 20sec

### Changed

- Adaptation of the top-level navigation
- The user is informed if the started TAS version is still blocked by an older instance
- The link to the downloads on the product website is country-specific
- Further differentiation in the address mode between rotary switches and dip switches
- Adaptation of the design of the web pages

### Fixed

- Updated some text messages and tooltips
- Repeated capturing of the same HF tag is not indicated
- Incorrect block transfer with inconsistent parameter sets
- Incorrect redirection to the device web page after IP address changes or a reset

## Changelog version 1.8.1.0

### Fixed

- Supports Reader ID for TN-UHF-Q180L300-AUS-CDS and TN-UHF-Q300-AUS-CDS

## Changelog version 1.8.0.0

### Added

- Switching language to German
- New Radar Monitor 2.0 with angle measurement
- Magnet Monitor to represent the magnetic field strength in all three axes as well as the magnitude vector and sum vector
- Exports configuration from connected IO-Link devices
- Imports configuration into one or several connected IO-Link devices in a batch
- Sets Real Time Clock to one or several devices in a batch
- Supports use of network card with several IP addresses
- Supports firmware updates for devices with old firmware version within 180 seconds, after a power reset has been performed
- Supports open device webserver for devices with old firmware
- Shows Turck cloud settings in TAS
- Exports or prints list of scanned UIDs of HF Tags

### Changed

- Global password can be set or deleted via action in the toolbar
- Run firmware updates via the single device actions
- Device name added in IO-Link view
- Information on waiting time issued after download of a ARGEE program
- Some icons replaced and reordered
- Entry of a valid subnet mask checked
- Shows EtherNet/IP and Modbus TCP mapping in GEN device documentation, if the station is configured without connected hardware

### Fixed

- Reloading of "IODD Configurator - Observation Tab" after changing parameters
- Some text messages and tooltips updated
- Supports firmware updates for all hardware versions of TBEN-L…-8IOL
- Incorrect assignment of ID and device type for Q300
- IODD Configurator: Parameters that control the scope of process data are also supported under "Observation".
- Under the GEN device documentation a diagnostic word is to be considered in the EtherNet/IP mapping if the slot is configured as 'empty slot' and is located within the module list

## Changelog version 1.7.0.0

### Added

- IO-Link View:
  - Scans and views Turck IO-Link masters and all connected IO-Link devices in the network
  - Gets specific information about connected IO-Link devices
  - Executes specific device actions, like Wink, open IO-Link Master in TAS, open IODD Configurator and IO-Link device monitor
  - Filters for specific IO-Link devices
- RFID Tag Actions HF:
  - Scans UIDs of HF tags and creates a list
  - Gets tag information about tag type, memory size and supported features
  - Reads tag memory in Hex and ASCII
  - Edits data and writes to tag in Hex
  - Sets specific data to the complete or a selected memory area of the tag
- Diagnostic report to export or print all device settings, status and diagnostics
- Configuration mode for inductive coupler with IO-link
- Additional plot for suppression FFT in the Radar Monitor
- Checks and informs if an addressing conflict occured for the used network adapters
- Supports factory reset, sets IP address and accesses system settings of TX devices
- Supports new hardware version of BL20-E-GW-EN and BL67-GW-EN
- Supports to “go online” with a device automatically, if it isn´t connected to a plc
- Supports to activate Force Mode to get access to the device, if it is connected to a plc

### Changed

- Improved update process of TAS, which replace the files, stops the old TAS instance and restarts new version of TAS automatically
- Changes default settings in RFID application “Tag Trace”
- Devices with running ARGEE or CODESYS programs supports edit device, reset and firmware update
- Uncheck the import of unique device data by default

### Fixed

- Prevents that process data won´t be updated by using the USB IO-Link Master
- Size of the navigation bar changed
- Some text messages and tooltips updated

## Initial version 1.6.0.0